4.3. Start Capturing
Prev | Chapter 4. Capturing Live Network Data | Next

## 4.3. Start Capturing

One of the following methods can be used to start capturing packets with Wireshark:

- You can get an overview of the available local interfaces using the " Capture Interfaces" dialog box, see Figure 4.1, “The "Capture Interfaces" dialog box on Microsoft Windows” or Figure 4.2, “The "Capture Interfaces" dialog box on Unix/Linux”. You can start a capture from this dialog box, using (one of) the "Capture" button(s).

- You can start capturing using the " Capture Options" dialog box, see Figure 4.3, “The "Capture Options" dialog box”.

- If you have selected the right capture options before, you can immediately start a capture using the " Capture Start" menu / toolbar item. The capture process will start immediately.

- If you already know the name of the capture interface, you can start Wireshark from the command line and use the following:

      wireshark -i eth0 -k

  This will start Wireshark capturing on interface eth0, more details can be found at: Section 9.2, “Start Wireshark from the command line”.

Prev | Up | Next
4.2. Prerequisites | Home | 4.4. The "Capture Interfaces" dialog box