4.7. Capture files and file modes
Prev | Chapter 4. Capturing Live Network Data | Next

## 4.7. Capture files and file modes

While capturing, the underlying libpcap capturing engine will grab the packets from the network card and keep the packet data in a (relatively) small kernel buffer. This data is read by Wireshark and saved into the capture file(s) the user specified.

Different modes of operation are available when saving this packet data to the capture file(s).

| Tip!
Working with large files (several 100 MB's) can be quite slow. If you plan to do a long term capture or capturing from a high traffic network, think about using one of the "Multiple files" options. This will spread the captured packets over several smaller files which can be much more pleasant to work with.

| Note!
Using Multiple files may cut context related information. Wireshark keeps context information of the loaded packet data, so it can report context related problems (like a stream error) and keeps information about context related protocols (e.g. where data is exchanged at the establishing phase and only referred to in later packets). As it keeps this information only for the loaded file, using one of the multiple file modes may cut these contexts. If the establishing phase is saved in one file and the things you would like to see is in another, you might not see some of the valuable context related information.

| Tip!
Information about the folders used for the capture file(s), can be found in Appendix A, Files and Folders.

Table 4.1. Capture file mode selected by capture options

"File" option | "Use multiple files" option | "Ring buffer with n files" option | Mode | Resulting filename(s) used
--- | --- | --- | --- | ---
- | - | - | Single temporary file | etherXXXXXX (where XXXXXX is a unique number)
foo.cap | - | - | Single named file | foo.cap
foo.cap | x | - | Multiple files, continuous | foo_00001_20040205110102.cap, foo_00002_20040205110102.cap, ...
foo.cap | x | x | Multiple files, ring buffer | foo_00001_20040205110102.cap, foo_00002_20040205110102.cap, ...

Single temporary file

  A temporary file will be created and used (this is the default). After the capturing is stopped, this file can be saved later under a user specified name.

Single named file

  A single capture file will be used. If you want to place the new capture file to a specific folder, choose this mode.

Multiple files, continuous

  Like the "Single named file" mode, but a new file is created and used, after reaching one of the multiple file switch conditions (one of the "Next file every ..." values).

Multiple files, ring buffer

  Much like "Multiple files continuous", reaching one of the multiple files switch conditions (one of the "Next file every ..." values) will switch to the next file. This will be a newly created file if value of "Ring buffer with n files" is not reached, otherwise it will replace the oldest of the formerly used files (thus forming a "ring").

  This mode will limit the maximum disk usage, even for an unlimited amount of capture input data, keeping the latest captured data.

Prev | Up | Next
4.6. The "Interface Details" dialog box | Home | 4.8. Link-layer header type