9.11. SCCP users Table
Prev | Chapter 9. Customizing Wireshark | Next

## 9.11. SCCP users Table

Wireshark uses this table to map specific protocols to a certain DPC/SSN combination for SCCP.

This table is handled by an Section 9.7, “User Table” with the following fields.

ni

  An Integer representing the network indicator for which this association is valid.

called_pc

  An range of integers representing the dpcs for which this association is valid.

called_ssn

  An range of integers representing the ssns for which this association is valid.

user

  The protocol that is carried over this association

Prev | Up | Next
9.10. Tektronix K12xx/15 RF5 protocols Table | Home | 9.12. SMI (MIB and PIB) Modules